{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":94,"n_cols":7,"rows_kept":94,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTM-R"]
[]
[]
[]
[]
["","","","","","FTXTM30R2V1B","FTXTM40R2V1B"]
["Skaņas spiediena līmenis","Apsilde","","Augsta","dBA","45.0"]
["","","","Vidēja","dBA","31.0"]
["","","","Klusa darbība","dBA","19.0"]
["","","","Zema","dBA","22.0"]
["","Dzesēšana","","Vidēja","dBA","33.0"]
["","","","Klusa darbība","dBA","21.0"]
["","","","Zema","dBA","25.0"]
["","","","Augsta","dBA","45.0"]
["Standard Accessories","Uzstādīšanas rokasgrāmata","","","","1"]
["","Lietošanas rokasgrāmata","","","","1"]
["","Bezvadu tālvadības pults","","","","1"]
["","AAA sausās baterijas","","","","2"]
["","Tālvadības turētājs","","","","1"]
["","Montāžas plāksne","","","","1"]
["","Iekštelpu ierīces fiksācijas skrūves","","","","2"]
["","Sudraba daļiņu filtrs","","","","1"]
["Vadības sistēmas","Tālv. pults ar vadu","","","","BRC073A1"]
["","Infrared remote control","","","","ARC466A75"]
["Cauruļu savienojumi","Šķidrums","","OD","mm","6.35"]
["","Gāze","","OD","mm","9.50"]
["","Izplūde","","","","18"]
["Power input","Dzesēšana","","Nom.","kW","0.035"]
["","Apsilde","","Nom.","kW","0.039"]
["Sound power level","Dzesēšana","","","dBA","60.0"]
["","Apsilde","","","dBA","61.0"]
["Izmēri","Ierīce","","Platums","mm","778"]
["","","","Dziļums","mm","272"]
["","","","Augstums","mm","295"]
["Korpuss","Krāsa","","","","Balts"]
["Svars","Ierīce","","","kg","10.0"]
["Ventilators","Gaisa plūsmas ātrums","Apsilde","Augsta","m³/min.","12.5"]
["","","","Zema","m³/min.","4.9"]
["","","","Vidēja","m³/min.","7.5"]
["","","","Klusa darbība","m³/min.","4.0"]
["","","Dzesēšana","Zema","m³/min.","5.3"]
["","","","Vidēja","m³/min.","7.8"]
["","","","Augsta","m³/min.","12.2"]
["","","","Klusa darbība","m³/min.","4.1"]
["Power supply","Fāze","","","","1~"]
["","Frekvence","","","Hz","50"]
["","Nosaukums","","","","V1"]
["","Spriegums","","","V","220-240"]
["Notes","","","","","(1) - Dzesēšana: iekšējā temp. 27 °CDB,19,0 °CWB; ārējā temp. 35 °CDB, 24 °CWB; ekvivalentais cauruļvadu garums: 5 m"]
["","","","","","(2) - Apsilde: iekšējā temp. 20 °CDB; ārējā temp. 7 °CDB, 6 °CWB; ekvivalentā dzesēšanas cauruļvadu sistēma: 5 m"]
["","","","","","(3) - Elektrības datus skatiet atsevišķos zīmējumos"]
["Strāvas ievade","Dzesēšana","","Nom.","kW","","0.053"]
["","Apsilde","","Nom.","kW","","0.06"]
["Korpuss","Krāsa","","","","","Balts"]
["Izmēri","Ierīce","","Augstums","mm","","299"]
["","","","Platums","mm","","998"]
["","","","Dziļums","mm","","292"]
["Svars","Ierīce","","","kg","","14.5"]
["Ventilators","Gaisa plūsmas ātrums","Dzesēšana","Augsta","m³/min.","","15.4"]
["","Gaisa caurplūde","Dzesēšana","Vidēja","m³/min.","","9.5"]
["","","","Zema","m³/min.","","5.8"]
["","","","Klusa darbība","m³/min.","","4.6"]
["","","Apsilde","Augsta","m³/min.","","17.5"]
["","Gaisa caurplūde","Apsilde","Vidēja","m³/min.","","10.5"]
["","","Apsilde","Zema","m³/min.","","7.1"]
["","","","Klusa darbība","m³/min.","","5.9"]
["Skaņas jaudas līmenis","Dzesēšana","","","dBA","","60"]
["","Apsilde","","","dBA","","61"]
["Skaņas spiediena līmenis","Dzesēšana","","Augsta","dBA","","46"]
["","","","Vidēja","dBA","","32"]
["","","","Zema","dBA","","24"]
["","","","Klusa darbība","dBA","","20"]
["","Apsilde","","Augsta","dBA","","46"]
["","","","Vidēja","dBA","","31"]
["","","","Zema","dBA","","22"]
["","","","Klusa darbība","dBA","","19"]
["Cauruļu savienojumi","Šķidrums","","OD","mm","","6.35"]
["","Gāze","","OD","mm","","9.5"]
["","Aizplūde","","","","","18"]
["Vadības sistēmas","Infrared remote control","","","","","ARC466A75"]
["Vadības sistēmas","Tālv. pults ar vadu","","","","","BRC073A1"]
["Standard Accessories","Installation manual","","","","","1"]
["","Wireless remote control","","","","","1"]
["","AAA dry-cell batteries","","","","","2"]
["","Operation manual","","","","","1"]
["","Titanium apatite deodorizing filter","","","","","1"]
["","Silver particle filter","","","","","1"]
["","Indoor unit fixing screws","","","","","2"]
["","Mounting plate","","","","","1"]
["","Remote control holder","","","","","1"]
["Barošanas avots","Nosaukums","","","","","V1"]
["","Fāze","","","","","1~"]
["Strāvas padeve","Frekvence","","","Hz","","50"]
["","Spriegums","","","V","","220-240"]