{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":47,"n_cols":7,"rows_kept":47,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTM-S"]
[]
[]
[]
[]
["","","","","","FTXTM30S2V1B","FTXTM40S2V1B"]
["Strāvas ievade","Dzesēšana","","Nom.","kW","0.035","0.053"]
["","Apsilde","","Nom.","kW","0.039","0.06"]
["Korpuss","Krāsa","","","","Balts","Balts"]
["Izmēri","Ierīce","","Augstums","mm","295","299"]
["","","","Platums","mm","778","998"]
["","","","Dziļums","mm","272","292"]
["Svars","Ierīce","","","kg","10","15"]
["Ventilators","Gaisa plūsmas ātrums","Dzesēšana","Augsta","m³/min.","11.5","15.1"]
["","Gaisa caurplūde","Dzesēšana","Vidēja","m³/min.","7.5","9.2"]
["","","","Zema","m³/min.","5.2","5.6"]
["","","","Klusa darbība","m³/min.","4.2","4.8"]
["","","Apsilde","Augsta","m³/min.","11.6","17"]
["","Gaisa caurplūde","Apsilde","Vidēja","m³/min.","7.3","10"]
["","","Apsilde","Zema","m³/min.","4.7","6"]
["","","","Klusa darbība","m³/min.","4","5.1"]
["Skaņas jaudas līmenis","Dzesēšana","","","dBA","60","60"]
["","Apsilde","","","dBA","60","60"]
["Skaņas spiediena līmenis","Dzesēšana","","Augsta","dBA","45","46"]
["","","","Vidēja","dBA","33","32"]
["","","","Zema","dBA","25","24"]
["","","","Klusa darbība","dBA","21","20"]
["","Apsilde","","Augsta","dBA","45","46"]
["","","","Vidēja","dBA","31","31"]
["","","","Zema","dBA","22","22"]
["","","","Klusa darbība","dBA","19","19"]
["Aukstumaģents","GWP","","","","675","675"]
["Cauruļu savienojumi","Šķidrums","","OD","mm","6.35","6.35"]
["","Gāze","","OD","mm","9.5","9.5"]
["","Aizplūde","","","","18","18"]
["Vadības sistēmas","Infrasarkano staru tālv. pults","","","","ARC466A83","ARC466A83"]
["","Tālv. pults ar vadu","","","","BRC073A1","BRC073A1"]
["Standard Accessories","Installation manual","","","","1","1"]
["","Wireless remote control","","","","1","1"]
["","AAA dry-cell batteries","","","","2","2"]
["","General safety precautions","","","","1","1"]
["","Silver particle filter","","","","1","1"]
["","Remote control holder","","","","1","1"]
["","Screw bag","","","","1","1"]
["Barošanas avots","Fāze","","","","1~","1~"]
["Strāvas padeve","Frekvence","","","Hz","50","50"]
["","Spriegums","","","V","220-240","220-240"]