{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":83,"n_cols":7,"rows_kept":83,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTP-K"]
[]
[]
[]
[]
["","","","","","FTXTP25K3V1B","FTXTP35K3V1B"]
["Skaņas spiediena līmenis","Apsilde","","Augsta","dBA","43"]
["","","","Vidēja","dBA","35"]
["","","","Klusa darbība","dBA","21"]
["","","","Zema","dBA","26"]
["","Dzesēšana","","Vidēja","dBA","35"]
["","","","Klusa darbība","dBA","21"]
["","","","Zema","dBA","26"]
["","","","Augsta","dBA","43"]
["Standard Accessories","Uzstādīšanas rokasgrāmata","","","","1"]
["","Lietošanas rokasgrāmata","","","","1"]
["","Bezvadu tālvadības pults","","","","1"]
["","AAA sausās baterijas","","","","2"]
["","Tālvadības turētājs","","","","1"]
["","Montāžas plāksne","","","","1"]
["","Titāna apatīta dezodorējošais filtrs","","","","2"]
["","Iekštelpu ierīces fiksācijas skrūves","","","","2"]
["Vadības sistēmas","Tālv. pults ar vadu","","","","BRC944B2, BRC073A1"]
["","Infrared remote control","","","","ARC480A11"]
["Cauruļu savienojumi","Šķidrums","","OD","mm","6.35"]
["","Gāze","","OD","mm","9.50"]
["","Izplūde","","","","16 (pievienošanas šļūtenes iekšējais diametrs)"]
["Strāvas ievade","Dzesēšana","","Nom.","kW","0.030"]
["","Apsilde","","Nom.","kW","0.035"]
["Skaņas jaudas līmenis","Dzesēšana","","","dBA","58"]
["","Apsilde","","","dBA","58"]
["Izmēri","Ierīce","","Platums","mm","770"]
["","","","Dziļums","mm","225"]
["","","","Augstums","mm","285"]
["Korpuss","Krāsa","","","","Balts"]
["Svars","Ierīce","","","kg","9.0"]
["Power supply","Phase","","","","1~"]
["","Frekvence","","","Hz","50"]
["","Nosaukums","","","","V1"]
["","Spriegums","","","V","220-240"]
["Notes","","","","","(1) - Elektrības datus skatiet atsevišķā zīmējumā"]
["Strāvas ievade","Dzesēšana","","Nom.","kW","","0.03"]
["","Apsilde","","Nom.","kW","","0.035"]
["Korpuss","Krāsa","","","","","Balts"]
["Izmēri","Ierīce","","Augstums","mm","","285"]
["","","","Platums","mm","","770"]
["","","","Dziļums","mm","","225"]
["Svars","Ierīce","","","kg","","9"]
["Ventilators","Gaisa plūsmas ātrums","Dzesēšana","Augsta","m³/min.","","11.4"]
["","Gaisa caurplūde","Dzesēšana","Vidēja","m³/min.","","8.2"]
["","","","Zema","m³/min.","","5.4"]
["","","","Klusa darbība","m³/min.","","4.3"]
["","","Apsilde","Augsta","m³/min.","","10.8"]
["","Gaisa caurplūde","Apsilde","Vidēja","m³/min.","","7.8"]
["","","Apsilde","Zema","m³/min.","","5.8"]
["","","","Klusa darbība","m³/min.","","4.9"]
["Skaņas jaudas līmenis","Dzesēšana","","","dBA","","58"]
["","Apsilde","","","dBA","","58"]
["Skaņas spiediena līmenis","Dzesēšana","","Augsta","dBA","","43"]
["","","","Vidēja","dBA","","35"]
["","","","Zema","dBA","","26"]
["","","","Klusa darbība","dBA","","21"]
["","Apsilde","","Augsta","dBA","","43"]
["","","","Vidēja","dBA","","35"]
["","","","Zema","dBA","","26"]
["","","","Klusa darbība","dBA","","21"]
["Cauruļu savienojumi","Šķidrums","","OD","mm","","6.35"]
["","Gāze","","OD","mm","","9.5"]
["","Aizplūde","","","","","16 (pievienošanas šļūtenes iekšējais diametrs)"]
["Vadības sistēmas","Infrared remote control","","","","","ARC480A11"]
["Vadības sistēmas","Tālv. pults ar vadu","","","","","BRC944B2, BRC073A1"]
["Standard Accessories","Installation manual","","","","","1"]
["","Wireless remote control","","","","","1"]
["","AAA dry-cell batteries","","","","","2"]
["","Operation manual","","","","","1"]
["","Titanium apatite deodorizing filter","","","","","2"]
["","Indoor unit fixing screws","","","","","2"]
["","Mounting plate","","","","","1"]
["","Remote control holder","","","","","1"]
["Barošanas avots","Nosaukums","","","","","V1"]
["","Fāze","","","","","1~"]
["Strāvas padeve","Frekvence","","","Hz","","50"]
["","Spriegums","","","V","","220-240"]