{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":8,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXZ-N"]
[]
[]
[]
[]
["","","","","","FTXZ25NV1B","FTXZ35NV1B","FTXZ50NV1B"]
["Skaņas spiediena līmenis","Apsilde","","Augsta","dBA","39","42","44"]
["","","","Klusa darbība","dBA","19","19","24"]
["","","","Zema","dBA","28","29","31"]
["","Dzesēšana","","Klusa darbība","dBA","19","19","23"]
["","","","Zema","dBA","26","27","30"]
["","","","Augsta","dBA","38","42","47"]
["","","","Nom.","dBA","35","36","38"]
["","Dzesēšana","","Nom.","dBA","33","35","38"]
["Standard Accessories","Fotokatalītisks gaisu attīrošs un dezodorējošs filtrs","","","","1","1","1"]
["","Bezvadu tālvadības pults","","","","1","1","1"]
["","Sausie akumulatori","","","","2","2","2"]
["","Tālvadības turētājs","","","","1","1","1"]
["","Iekštelpu ierīces fiksācijas skrūves","","","","3","3","3"]
["","Montāžas plāksne","","","","1","1","1"]
["Vadības sistēmas","Infrared remote control","","","","ARC477A1","ARC477A1","ARC477A1"]
["Cauruļu savienojumi","Šķidrums","","OD","mm","6.35","6.35","6.35"]
["","Gāze","","OD","mm","9.5","9.5","9.5"]
["Power input","Dzesēšana","","Nom.","kW","0.030","0.030","0.030"]
["","Apsilde","","Nom.","kW","0.030","0.030","0.030"]
["Sound power level","Dzesēšana","","","dBA","54","57","60"]
["","Apsilde","","","dBA","56","57","59"]
["Izmēri","Ierīce","","Platums","mm","798","798","798"]
["","","","Dziļums","mm","372","372","372"]
["","","","Augstums","mm","295","295","295"]
["Korpuss","Krāsa","","","","Balts","Balts","Balts"]
["Svars","Ierīce","","","kg","15","15","15"]
["Ventilators","Gaisa plūsmas ātrums","Apsilde","Augsta","m³/min.","11.7","13.3","14.4"]
["","","","Zema","m³/min.","6.7","6.9","7.7"]
["","","","Klusa darbība","m³/min.","4.8","4.8","5.9"]
["","","Dzesēšana","Zema","m³/min.","5.3","5.6","6.6"]
["","","","Augsta","m³/min.","10.7","12.1","15.0"]
["","","","Klusa darbība","m³/min.","4.0","4.0","4.6"]
["","","","Nom.","m³/min.","8.6","9.2","10.7"]
["","","Dzesēšana","Nom.","m³/min.","7.5","8.4","9.2"]
["Power supply","Fāze","","","","1~","1~","1~"]
["","Nosaukums","","","","V1","V1","V1"]
["","Frekvence","","","Hz","50","50","50"]
["","Spriegums","","","V","220-240","220-240","220-240"]
["Notes","","","","","(1) - 220 V","(1) - 220 V","(1) - 220 V"]
["","","","","","(2) - 230 V","(2) - 230 V","(2) - 230 V"]
["","","","","","(3) - 240 V","(3) - 240 V","(3) - 240 V"]
["","","","","","(4) - Siltummaiņa priekšpuse","(4) - Siltummaiņa priekšpuse","(4) - Siltummaiņa priekšpuse"]
["","","","","","(5) - Siltummaiņa aizmugure","(5) - Siltummaiņa aizmugure","(5) - Siltummaiņa aizmugure"]