{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":16,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FUA-A / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FUA100AVEB / RZQG100L8Y1B","FUA125AVEB / RZQG125L8Y1B","FUA71AVEB / FUA71AVEB / RZQG100L8Y1B","FUA71AVEB / FUA71AVEB / RZQG125L8Y1B","FUA100AVEB9 / RZQG100L8Y1B","FUA125AVEB9 / RZQG125L8Y1B","FUA71AVEB9 / FUA71AVEB9 / RZQG100L8Y1B","FUA71AVEB9 / FUA71AVEB9 / RZQG125L8Y1B","FUA100AVEB / RZQG71L8Y1B","FUA71AVEB9 / RZQG71L8Y1B","FUA100AVEB9 / RZQG71L8Y1B","FUA71AVEB / RZQG71L8Y1B"]
["Energoefektivitātes diapazons","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Dzesēšanas jauda","Nom.","","kW","","","","","","","","","6.80","6.80","6.80","6.80"]
["Telpas dzesēšana","SEER","","","","","","","","","","","6.42","6.42","6.42","6.42"]
["","Gada enerģijas patēriņš","","kWh/a","","","","","","","","","371","371","371","371"]
["","Jauda","Pdesign","kW","","","","","","","","","6.80","6.80","6.80","6.80"]
["","Energoefektivitātes klase","","","","","","","","","","","A++","A++","A++","A++"]
["Telpu apsilde (mērens klimats)","Jauda","Pdesign","kW","","","","","","","","","7.60","7.60","7.60","7.60"]
["","SCOP/A","","","","","","","","","","","4.20","4.20","4.20","4.20"]
["","Energoefektivitātes klase","","","","","","","","","","","A+","A+","A+","A+"]
["","Gada enerģijas patēriņš","","kWh/a","","","","","","","","","2,534","2,534","2,534","2,534"]
["Nominālā efektivitāte","EER","","","","","","","","","","","4.07","4.07","4.07","4.07"]
["Notes","","","","","","","","","","","","(1) - Darbības diapazonu skatiet atsevišķā attēlā","(1) - Nominālā dzesēšanas jauda noteikta, pamatojoties uz: iekštelpu temperatūru: 27°CDB, 19°CWB, āra temperatūru: 35°CDB; ekvivalentā dzesēšanas cauruļvadu sistēma: 5 m, līmeņa atšķirība: 0 m.","(1) - Darbības diapazonu skatiet atsevišķā attēlā","(1) - Nominālā dzesēšanas jauda noteikta, pamatojoties uz: iekštelpu temperatūru: 27°CDB, 19°CWB, āra temperatūru: 35°CDB; ekvivalentā dzesēšanas cauruļvadu sistēma: 5 m, līmeņa atšķirība: 0 m."]
["","","","","","","","","","","","","(2) - Elektrības datus skatiet atsevišķā zīmējumā","(2) - Nominālās apsildes jaudas balstās uz: iekštelpas temperatūru: 20°CDB, ārējo temperatūru: 7°CDB, 6°CWB, ekvivalentā dzesētāja cauruļvadu sistēma: 5m, līmeņa atšķirība: 0 m.","(2) - Elektrības datus skatiet atsevišķā zīmējumā","(2) - Nominālās apsildes jaudas balstās uz: iekštelpas temperatūru: 20°CDB, ārējo temperatūru: 7°CDB, 6°CWB, ekvivalentā dzesētāja cauruļvadu sistēma: 5m, līmeņa atšķirība: 0 m."]
["Nominālā efektivitāte","Gada enerģijas patēriņš","","kWh","","","","","","","","","","835","","835"]
["","COP","","","","","","","","","","","","4.08","","4.08"]
["","Enerģijas marķēšanas direktīva","Dzesēšana","","","","","","","","","","","A","","A"]
["","","Apsilde","","","","","","","","","","","A","","A"]
["Apsildes jauda","Nom.","","kW","","","","","","","","","","7.50","","7.50"]
["Notes","","","","","","","","","","","","","(3) - Darbības diapazonu skatiet atsevišķā attēlā","","(3) - Darbības diapazonu skatiet atsevišķā attēlā"]
["","","","","","","","","","","","","","(4) - Elektrības datus skatiet atsevišķā zīmējumā","","(4) - Elektrības datus skatiet atsevišķā zīmējumā"]