{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":82,"n_cols":11,"rows_kept":82,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FUA-A"]
[]
[]
[]
[]
["","","","","","FUA71AVEB9","FUA100AVEB9","FUA125AVEB9","FUA71AVEB (Archived)","FUA100AVEB (Archived)","FUA125AVEB (Archived)"]
["Skaņas spiediena līmenis","Apsilde","","Augsta","dBA","","","","41","46","47"]
["","","","Vidēja","dBA","","","","38","42","43"]
["","","","Zema","dBA","","","","35","39","40"]
["","Dzesēšana","","Vidēja","dBA","","","","38","42","43"]
["","","","Zema","dBA","","","","35","39","40"]
["","","","Augsta","dBA","","","","41","46","47"]
["Standard Accessories","Lietošanas rokasgrāmata","","","","","","","1","1","1"]
["","Uzstādīšanas rokasgrāmata","","","","","","","1","1","1"]
["","Izplūdes šļūtene","","","","","","","1","1","1"]
["","Termiskās izolācijas caurule","","","","","","","3","3","3"]
["","Sasienamie iesaiņojumi","","","","","","","10","10","10"]
["","Šļūtenes apkava","","","","","","","1","1","1"]
["","Blīvējamais materiāls","","","","","","","4","4","4"]
["","Paplāksnes fiksācijas plāksne","","","","","","","1","1","1"]
["","Izplūdes savienojums","","","","","","","1","1","1"]
["","Neausts materiāls","","","","","","","1","1","1"]
["","Paplāksne","","","","","","","8","8","8"]
["","Izplūdes šļūtenes fiksācijas skrūve","","","","","","","5","5","5"]
["Vadības sistēmas","Wired remote control","","","","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Dzesēšanas jauda","Kopējā jauda","","Nom.","kW","","","","","","12.1"]
["Cauruļvadu savienojumi","Šķidrums","","OD","mm","","","","9.52","9.52","9.52"]
["","Gāze","","OD","mm","","","","15.9","15.9","15.9"]
["","Izplūde","","","","","","","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)"]
["Sound power level","Dzesēšana","","","dBA","","","","59","64","65"]
["","Apsilde","","","dBA","","","","59","64"]
["Izmēri","Ierīce","","Platums","mm","","","","950","950","950"]
["","","","Dziļums","mm","","","","950","950","950"]
["","","","Augstums","mm","","","","198","198","198"]
["Korpuss","Materiāls","","","","","","","Mastika","Mastika","Mastika"]
["","Krāsa","","","","","","","Dzidri balts","Dzidri balts","Dzidri balts"]
["Svars","Ierīce","","","kg","","","","25.0","26.0","26"]
["Ventilators","Gaisa plūsmas ātrums","Apsilde","Augsta","m³/min.","","","","23.0","31.0","32.5"]
["","","","Vidēja","m³/min.","","","","19.5","25.5","26.5"]
["","","","Zema","m³/min.","","","","16.0","20.0","20.5"]
["","","Dzesēšana","Zema","m³/min.","","","","16.0","20.0","20.5"]
["","","","Vidēja","m³/min.","","","","19.5","25.5","26.5"]
["","","","Augsta","m³/min.","","","","23.0","31.0","32.5"]
["Novadīšanas augstums","mm","","","","","","","600","600","600"]
["Apsildes jauda","Kopējā jauda","","Nom.","kW","","","","","","13.5"]
["Korpuss","Krāsa","","","","Dzidri balts","Dzidri balts","Dzidri balts"]
["","Materiāls","","","","Mastika","Mastika","Mastika"]
["Izmēri","Ierīce","","Augstums","mm","198","198","198"]
["","","","Platums","mm","950","950","950"]
["","","","Dziļums","mm","950","950","950"]
["Svars","Ierīce","","","kg","25.0","26.0","26.0"]
["Ventilators","Gaisa plūsmas ātrums","Dzesēšana","Augsta","m³/min.","23.0","31.0","32.5"]
["","Gaisa caurplūde","Dzesēšana","Vidēja","m³/min.","19.5","25.5","26.5"]
["","","","Zema","m³/min.","16.0","20.0","20.5"]
["","","Apsilde","Augsta","m³/min.","23.0","31.0","32.5"]
["","Gaisa caurplūde","Apsilde","Vidēja","m³/min.","19.5","25.5","26.5"]
["","","Apsilde","Zema","m³/min.","16.0","20.0","20.5"]
["Skaņas jaudas līmenis","Dzesēšana","","","dBA","59","64","65"]
["Skaņas spiediena līmenis","Dzesēšana","","Augsta","dBA","41","46","47"]
["","","","Vidēja","dBA","38","42","43"]
["","","","Zema","dBA","35","39","40"]
["","Apsilde","","Augsta","dBA","41","46","47"]
["","","","Vidēja","dBA","38","42","43"]
["","","","Zema","dBA","35","39","40"]
["Cauruļu savienojumi","Šķidrums","","OD","mm","9.52","9.52","9.52"]
["","Gāze","","OD","mm","15.9","15.9","15.9"]
["","Aizplūde","","","","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)"]
["Novadīšanas augstums","mm","","","","600","600","600"]
["Standard Accessories","Installation manual","","","","1","1","1"]
["","Thermal insulation tube","","","","3","3","3"]
["","Non woven fabric","","","","1","1","1"]
["","Drain joint","","","","1","1","1"]
["","Hose band","","","","1","1","1"]
["","Operation manual","","","","1","1","1"]
["","Drain hose","","","","1","1","1"]
["","Fixing screw for drain hose","","","","5","5","5"]
["","Sealing material","","","","4","4","4"]
["","Tie-wraps","","","","10","10","10"]
["","Washer","","","","8","8","8"]
["","Washer fixing plate","","","","1","1","1"]
["Dzesēšanas jauda","Kopējā jauda","","Nom.","kW","","","12.10"]
["Apsildes jauda","Kopējā jauda","","Nom.","kW","","","13.5"]