{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":45,"n_cols":7,"rows_kept":45,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FUQ-C"]
[]
[]
[]
[]
["","","","","FUQ71CVEB","FUQ100CVEB","FUQ125CVEB"]
["Skaņas spiediena līmenis","Apsilde","Augsta","dBA","41","46","47"]
["","","Nom.","dBA","38","42","43"]
["","","Zema","dBA","35","39","40"]
["","Dzesēšana","Zema","dBA","35","39","40"]
["","","Augsta","dBA","41","46","47"]
["","","Nom.","dBA","38","42","43"]
["Standard Accessories","Uzstādīšanas rokasgrāmata","","","Uzstādīšanas rokasgrāmata","Uzstādīšanas rokasgrāmata","Uzstādīšanas rokasgrāmata"]
["","Lietošanas rokasgrāmata","","","Lietošanas rokasgrāmata","Lietošanas rokasgrāmata","Lietošanas rokasgrāmata"]
["","Atbilstības deklarācija","","","Atbilstības deklarācija","Atbilstības deklarācija","Atbilstības deklarācija"]
["","Izplūdes šļūtene","","","Izplūdes šļūtene","Izplūdes šļūtene","Izplūdes šļūtene"]
["","Metāla skava","","","Metāla skava","Metāla skava","Metāla skava"]
["","Kronšteina skavas paplāksne","","","Kronšteina skavas paplāksne","Kronšteina skavas paplāksne","Kronšteina skavas paplāksne"]
["","Skavas","","","Skavas","Skavas","Skavas"]
["","Savilcējskava","","","Savilcējskava","Savilcējskava","Savilcējskava"]
["","Savienojumu izolācijas un blīvējuma materiāls","","","Savienojumu izolācijas un blīvējuma materiāls","Savienojumu izolācijas un blīvējuma materiāls","Savienojumu izolācijas un blīvējuma materiāls"]
["","Līkums","","","Līkums","Līkums","Līkums"]
["","Uzstādīšanas paraugs","","","Uzstādīšanas paraugs","Uzstādīšanas paraugs","Uzstādīšanas paraugs"]
["","Aizargmateriāls","","","Aizargmateriāls","Aizargmateriāls","Aizargmateriāls"]
["","Caurule ar L veida locījumu","","","Caurule ar L veida locījumu","Caurule ar L veida locījumu","Caurule ar L veida locījumu"]
["","Skrūves","","","Skrūves","Skrūves","Skrūves"]
["","Neausts materiāls","","","Neausts materiāls","Neausts materiāls","Neausts materiāls"]
["Vadības sistēmas","Wired remote control","","","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B"]
["","Infrared remote control","","","BRC7C58","BRC7C58","BRC7C58"]
["Piping connections","Šķidrums","OD","mm","9.52","9.52","9.52"]
["","Gāze","OD","mm","15.9","15.9","15.9"]
["","Izplūde","","","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)"]
["Skaņas jaudas līmenis","Dzesēšana","","dBA","59","64","65"]
["","Apsilde","","dBA","59","64","65"]
["Izmēri","Ierīce","Platums","mm","950","950","950"]
["","","Dziļums","mm","950","950","950"]
["","","Augstums","mm","198","198","198"]
["Korpuss","Materiāls","","","Mastika","Mastika","Mastika"]
["","Colour","","","Dzidri balts","Dzidri balts","Dzidri balts"]
["Svars","Ierīce","","kg","25","26","26"]
["Novadīšanas augstums","mm","","","600","600","600"]
["Power supply","Phase","","","1~","1~","1~"]
["","Frekvence","","Hz","50/60","50/60","50/60"]
["","Nosaukums","","","VE","VE","VE"]
["","Spriegums","","V","220-240/220","220-240/220","220-240/220"]