{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":8,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVA-A / RZASG-MY1"]
[]
[]
[]
[]
["","","","","FVA100AMVEB / RZASG100M7Y1B","FVA125AMVEB / RZASG125M7Y1B","FVA140AMVEB / RZASG140M7Y1B","FVA71AMVEB / FVA71AMVEB / RZASG140M7Y1B"]
["Dzesēšanas jauda","Nom.","","kW","","12.1 (1)","13.4 (1)"]
["Telpu dzesēšana","Gada enerģijas patēriņš","","kWh/a","","1,314","1,428"]
["","Jauda","Pdesign","kW","","12.1","13.4"]
["Telpu apsilde (mērens klimats)","Jauda","Pdesign","kW","","6.00","7.80"]
["","Gada enerģijas patēriņš","","kWh/a","","2,308","2,866"]
["Apsildes jauda","Nom.","","kW","","13.5 (2)","15.5 (2)"]
["Dzesēšanas jauda","Nom.","","kW","9.5","","","13.4"]
["Apsildes jauda","Nom.","","kW","10.8","","","15.5"]
["Telpu dzesēšana","Energoefektivitātes klase","","","A+"]
["","Jauda","Pdesign","kW","9.5","","","13.4"]
["","SEER","","","5.72","","","7.71"]
["","Gada enerģijas patēriņš","","kWh/a","581","","","1043"]
["Telpu apsilde (mērens klimats)","Energoefektivitātes klase","","","A"]
["","Jauda","Pdesign","kW","6","","","7.80"]
["","SCOP/A","","","3.83","","","4.43"]
["","Gada enerģijas patēriņš","","kWh/a","2193","","","2467"]
["Telpu dzesēšana","SEER","","","","5.52","5.63"]
["Telpu apsilde (mērens klimats)","SCOP/A","","","","3.64","3.81"]
["Notes","","","","","(1) - Nominālā dzesēšanas jauda noteikta, pamatojoties uz: iekštelpu temp.: 27°CDB, 19°CWB, āra temperatūru: 35°CDB; ekvivalentā dzesēšanas cauruļvadu sistēma: 5 m, līmeņa atšķirība: 0 m.","(1) - Nominālā dzesēšanas jauda noteikta, pamatojoties uz: iekštelpu temp.: 27°CDB, 19°CWB, āra temperatūru: 35°CDB; ekvivalentā dzesēšanas cauruļvadu sistēma: 5 m, līmeņa atšķirība: 0 m.","(1) - Nominālā dzesēšanas jauda noteikta, pamatojoties uz: iekštelpu temp.: 27°CDB, 19°CWB, āra temperatūru: 35°CDB; ekvivalentā dzesēšanas cauruļvadu sistēma: 5 m, līmeņa atšķirība: 0 m."]
["","","","","","(2) - Nominālās apsildes jaudas balstās uz: iekštelpas temperatūru: 20°CDB, ārējo temperatūru: 7°CDB, 6°CWB, ekvivalentā dzesētāja cauruļvadu sistēma: 5m, līmeņa atšķirība: 0 m.","(2) - Nominālās apsildes jaudas balstās uz: iekštelpas temperatūru: 20°CDB, ārējo temperatūru: 7°CDB, 6°CWB, ekvivalentā dzesētāja cauruļvadu sistēma: 5m, līmeņa atšķirība: 0 m.","(2) - Nominālās apsildes jaudas balstās uz: iekštelpas temperatūru: 20°CDB, ārējo temperatūru: 7°CDB, 6°CWB, ekvivalentā dzesētāja cauruļvadu sistēma: 5m, līmeņa atšķirība: 0 m."]
["","","","","","(3) - Darbības diapazonu skatiet atsevišķā attēlā","(3) - Darbības diapazonu skatiet atsevišķā attēlā"]
["","","","","","(4) - Elektrības datus skatiet atsevišķā zīmējumā","(4) - Elektrības datus skatiet atsevišķā zīmējumā"]
["Energoefektivitātes diapazons","","","","","","","A+++ ~ D"]