{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":8,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVQ-C / RZQSG-LV1/LY1"]
[]
[]
[]
[]
["","","","","FVQ71CVEB / RZQSG71L2V1B","FVQ100CVEB / RZQSG100L7Y1B9","FVQ100CVEB / RZQSG100L7V1B","FVQ125CVEB / RZQSG125L7Y1B9"]
["Dzesēšanas jauda","Nom.","","kW","6.8","9.5","9.5","12.0"]
["Telpas dzesēšana","SEER","","","5.11","5.11","5.11","4.31"]
["","Gada enerģijas patēriņš","","kWh/a","466","650.685","650.685","975"]
["","Jauda","Pdesign","kW","6.80","9.50","9.50","12.00"]
["","Energoefektivitātes klase","","","A","A","A","C"]
["Telpu apsilde (mērens klimats)","Jauda","Pdesign","kW","6.33","7.60","7.60","7.60"]
["","SCOP/A","","","3.81","3.80","3.80","3.81"]
["","Energoefektivitātes klase","","","A","A","A","A"]
["","Gada enerģijas patēriņš","","kWh/a","2,327","2,799","2,799","2,791"]
["Nominālā efektivitāte","Gada enerģijas patēriņš","","kWh","1,059","1,480","1,480","2,135"]
["","EER","","","3.21","3.21","3.21","2.81"]
["","COP","","","3.61","3.61","3.61","3.41"]
["","Enerģijas marķēšanas direktīva","Dzesēšana","","A","A","A","C"]
["","","Apsilde","","A","A","A","B"]
["Apsildes jauda","Nom.","","kW","7.5","10.8","10.8","13.5"]
["Notes","","","","(1) - EER/COP saskaņā ar Eurovent 2012, lietošanai vienīgi ārpus ES","(1) - EER/COP saskaņā ar Eurovent 2012, lietošanai vienīgi ārpus ES","(1) - EER/COP saskaņā ar Eurovent 2012, lietošanai vienīgi ārpus ES","(1) - EER/COP saskaņā ar Eurovent 2012, lietošanai vienīgi ārpus ES"]
["","","","","(2) - Nominālā efektivitāte: dzesēšana pie 35°/27° nominālā jauda, apsilde pie 7°/20° nominālā jauda","(2) - Nominālā efektivitāte: dzesēšana pie 35°/27° nominālā jauda, apsilde pie 7°/20° nominālā jauda","(2) - Nominālā efektivitāte: dzesēšana pie 35°/27° nominālā jauda, apsilde pie 7°/20° nominālā jauda","(2) - Nominālā efektivitāte: dzesēšana pie 35°/27° nominālā jauda, apsilde pie 7°/20° nominālā jauda"]