{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":52,"n_cols":6,"rows_kept":52,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXTM-B"]
[]
[]
[]
[]
["","","","","","FVXTM30B2V1B"]
["Strāvas ievade","Dzesēšana","","Nom.","kW","0.02"]
["","Apsilde","","Nom.","kW","0.03"]
["Korpuss","Krāsa","","","","Balts"]
["Izmēri","Ierīce","","Augstums","mm","600"]
["","","","Platums","mm","750"]
["","","","Dziļums","mm","238"]
["Svars","Ierīce","","","kg","17"]
["Ventilators","Gaisa plūsmas ātrums","Dzesēšana","Augsta","m³/min.","9"]
["","Gaisa caurplūde","Dzesēšana","Vidēja","m³/min.","6.7"]
["","","","Zema","m³/min.","4.8"]
["","","","Klusa darbība","m³/min.","4"]
["","","Apsilde","Augsta","m³/min.","9.4"]
["","Gaisa caurplūde","Apsilde","Vidēja","m³/min.","6.8"]
["","","Apsilde","Zema","m³/min.","5.3"]
["","","","Klusa darbība","m³/min.","4"]
["Skaņas jaudas līmenis","Dzesēšana","","","dBA","53"]
["","Apsilde","","","dBA","53"]
["Skaņas spiediena līmenis","Dzesēšana","","Augsta","dBA","39"]
["","","","Vidēja","dBA","32"]
["","","","Zema","dBA","25"]
["","","","Klusa darbība","dBA","20"]
["","Apsilde","","Augsta","dBA","39"]
["","","","Vidēja","dBA","32"]
["","","","Zema","dBA","25"]
["","","","Klusa darbība","dBA","19"]
["Aukstumaģents","GWP","","","","675"]
["Cauruļu savienojumi","Šķidrums","","OD","mm","6.35"]
["","Gāze","","OD","mm","9.5"]
["","Aizplūde","","","","VP20 (I.D. 20/O.D. 26)"]
["Vadības sistēmas","Infrasarkano staru tālv. pults","","","","ARC466A90"]
["","Tālv. pults ar vadu","","","","BRC073A1"]
["Standard Accessories","Installation manual","","","","1"]
["","Wireless remote control","","","","1"]
["","AAA dry-cell batteries","","","","2"]
["","General safety precautions","","","","1"]
["","Operation manual","","","","1"]
["","Titanium apatite deodorizing filter","","","","2"]
["","Remote control holder","","","","1"]
["","Screw bag","","","","1"]
["Barošanas avots","Nosaukums","","","","V1"]
["","Fāze","","","","1~"]
["Strāvas padeve","Frekvence","","","Hz","50"]
["","Spriegums","","","V","220-240"]
["Notes","","","","","(1) - Dzesēšana: iekšējā temp. 27°CDB, 19°CWB; ārējā temp. 35 °CDB, 24 °CWB; ekvivalentais cauruļvadu garums: 5 m"]
["","","","","","(2) - Apsilde: iekšējā temp. 20 °CDB; ārējā temp. 7 °CDB, 6 °CWB; ekvivalentā dzesēšanas cauruļvadu sistēma: 5 m"]
["","","","","","(3) - Elektrības datus skatiet atsevišķā zīmējumā"]