{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":6,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","LRYEQ-AY"]
[]
[]
[]
[]
["","","","","","LRYEQ16A7Y1"]
["Standard Accessories","Uzstādīšanas rokasgrāmata","","","","1"]
["","Lietošanas rokasgrāmata","","","","1"]
["","Savienojuma cauruļvadi","","","","1"]
["","Dzesētāja uzlīme F gāzes regulācijai","","","","1"]
["","Dzesētāja padeves marķējums","","","","1"]
["","Vairākvalodu fluorinēto siltumnīcu gāzu marķējumi","","","","1"]
["Svars","Ierīce","","","kg","370"]
["Aukstumaģents","Charge","","","TCO2Eq","24.0"]
["","GWP","","","","2,087.5"]
["","Charge","","","kg","11.5"]
["","Tips","","","","R-410A"]
["Ventilatora motors","Jauda","","","W","750"]
["","Piedziņa","","","","Tiešais pārvads"]
["Siltummainis","Veids","","","","Šķērseniskā ribojuma spole"]
["Izmēri","Ierīce","","Platums","mm","1,240"]
["","","","Dziļums","mm","765"]
["","","","Augstums","mm","1,680"]
["Korpuss","Krāsa","","","","Ziloņkaula balts"]
["Ventilators","Tips","","","","Propellera ventilators"]
["","Gaisa plūsmas ātrums","Dzesēšana","Nom.","m³/min.","230"]
["","Daudzums","","","","2"]
["Power supply","Fāze","","","","3~"]
["","Frekvence","","","Hz","50"]
["","Spriegums","","","V","380-415"]
["Notes","","","","","(1) - Dzesēšanas prioritātes režīms: iekšējā temp. 27°CDB, 19°CWB; ārējā temp. 32 °CDB; cauruļvadu garums: 7,5m; līmeņa atšķirība: 0 m"]
["","","","","","(2) - Dzesēšanas prioritātes režīms: iztvaikošanas temp. -10°C; ārējā temp. 32 °CDB; iesūkšanas SH: 10 °C"]
["","","","","","(3) - 100 % siltuma atjaunošanas režīms: iekšējā temp. 20 °CDB; ārējā temp. 7 °CDB, 6 °CWB; dzesēšanas slodze 18 kW; cauruļvadu garums: 7,5m; līmeņa atšķirība: 0 m"]
["","","","","","(4) - Piesātinājuma temperatūra ekvivalenti iesūkšanas spiedienam (dzesēšanas puse): -10 °C (atdzesētā stāvoklī); iekštelpu gaisa kondicioniera savienojuma jauda: 10 HP, ja siltuma atjaunošana ir 100 %"]
["","","","","","(5) - Kompresors 1"]
["","","","","","(6) - Kompresors 2"]
["","","","","","(7) - Kompresors 3"]
["","","","","","(8) - Ierīces rūpnīcas slodze"]
["","","","","","(9) - Eļļas sifonu uzstādiet 5 m atstatumā no āra ierīces"]
["","","","","","(10) - Papildu informācijai skatīt darbības diapazonu attēlu"]
["","","","","","(11) - Sīkāku informāciju par standarta piederumiem meklējiet uzstādīšanas un lietošanas rokasgrāmatā"]
["","","","","","(12) - Satur fluorētas siltumnīcefekta gāzes"]