{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":63,"n_cols":6,"rows_kept":63,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","MCK55W"]
[]
[]
[]
[]
["","","","","","MCK55WVM"]
["Type","","","","","Mitrināšanas gaisa attīrītājs"]
["Izmantošana","","","","","Uz grīdas novietojama ierīce"]
["Korpuss","Krāsa","","","","Balts"]
["Izmēri","Ierīce","","Augstums","mm","700"]
["","","","Platums","mm","270"]
["","","","Dziļums","mm","270"]
["Svars","Ierīce","","","kg","9.5"]
["Piemērojamā telpas platība","m²","","","","41 (1), 82 (2)"]
["CADR","m³/h","","","","320"]
["Gaisa attīrīšanas darbība","Strāvas ievade","","Turbo","kW","0.056"]
["","","","M","kW","0.017"]
["","","","L","kW","0.010"]
["","","","Klusums","kW","0.007"]
["Mitrināšanas darbība","Strāvas ievade","","Turbo","kW","0.058"]
["","","","M","kW","0.019"]
["","","","L","kW","0.014"]
["","","","Klusums","kW","0.011"]
["","Ūdens tvertnes tilpums","","","l","2.7"]
["Skaņas spiediena līmenis","Gaisa attīrīšanas darbība","","Turbo","dBA","53.0"]
["","","","Vidēja","dBA","39.0"]
["","","","Zema","dBA","29.0"]
["","","","Klusums","dBA","19.0"]
["","Mitrināšanas darbība","","Turbo","dBA","53.0"]
["","","","Vidēja","dBA","39.0"]
["","","","Zema","dBA","33.0"]
["","","","Klusums","dBA","25.0"]
["Ventilators","Gaisa plūsmas ātrums","Gaisa attīrīšanas darbība","Turbo","m³/h","330"]
["","","","Vidēja","m³/h","192"]
["","","","Zema","m³/h","120"]
["","","","Klusums","m³/h","54"]
["","","Mitrināšanas darbība","Turbo","m³/h","330"]
["","","","Vidēja","m³/h","192"]
["","","","Zema","m³/h","144"]
["","","","Klusums","m³/h","102"]
["Putekļu savākšanas metode","","","","","Elektrostatiskais HEPA filtrs"]
["Dezodorēšanas metode","","","","","Flash streamer + dezodorējošais katalizators"]
["Standard Accessories","Operation manual","","","","1"]
["","Electrostatic HEPA filter","","","","1"]
["","Deodorising filter","","","","1"]
["","Caster","","","","4"]
["","Humidifying filter","","","","2"]
["","Remote control holder","","","","1"]
["","Remote control lid","","","","1"]
["Barošanas vads","Barošanas vads","","","","1.8"]
["Barošanas avots","Fāze","","","","1~"]
["Strāvas padeve","Strāvas padeve-=-Frekvence","","Frekvence","","50/60"]
["","Strāvas padeve-=-Spriegums","","Spriegums","","220-240/220-230"]
["Nepārtrauktā strāva","Gaisa attīrīšanas darbība","Nepārtrauktā strāva-=-Gaisa attīrīšanas darbība-=-Turbo","Turbo","","0.50"]
["","","Nepārtrauktā strāva-=-Gaisa attīrīšanas darbība-=-Vidēja","Vidēja","","0.19"]
["","","Nepārtrauktā strāva-=-Gaisa attīrīšanas darbība-=-Zema","Zema","","0.12"]
["","","Nepārtrauktā strāva-=-Gaisa attīrīšanas darbība-=-Klusums","Klusums","","0.09"]
["","Mitrināšanas darbība","Nepārtrauktā strāva-=-Mitrināšanas darbība-=-Turbo","Turbo","","0.50"]
["","","Nepārtrauktā strāva-=-Mitrināšanas darbība-=-Vidēja","Vidēja","","0.20"]
["","","Nepārtrauktā strāva-=-Mitrināšanas darbība-=-Zema","Zema","","0.15"]
["","","Nepārtrauktā strāva-=-Mitrināšanas darbība-=-Klusums","Klusums","","0.13"]
["Notes","","","","","(1) - Piemērojamā telpas platība ir atbilstoša iekārtas darbināšanai ar maksimālu ventilatora ātrumu (HH). Piemērojamā telpas platība norāda platību, kurā noteiktu putekļu daļiņu daudzumu var likvidēt 30 minūšu laikā. (JEM 1467)"]
["","","","","","(2) - Konvertēts uz NRCC standartiem no testu vērtībām saskaņā ar JEM1467."]