{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":54,"n_cols":6,"rows_kept":54,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","MCK70YV"]
[]
[]
[]
[]
["","","","","","MCK70YVM"]
["Veids","","","","","Mitrināšanas gaisa attīrītājs"]
["Izmantošana","","","","","Uz grīdas novietojama ierīce"]
["Korpuss","Krāsa","","","","Balts (N9. 0)"]
["Izmēri","Ierīce","","Augstums","mm","600 (5)"]
["","","","Platums","mm","395"]
["","","","Dziļums","mm","287"]
["Svars","Ierīce","","","kg","12.5"]
["Piemērojamā telpas platība","m²","","","","48 (1), 96 (2)"]
["CADR","m³/h","","","","375"]
["Gaisa attīrīšanas darbība","Strāvas ievade","","Turbo","kW","0.066"]
["","","","M","kW","0.016"]
["","","","L","kW","0.01"]
["","","","Klusums","kW","0.008"]
["Mitrināšanas darbība","Strāvas ievade","","Turbo","kW","0.068"]
["","","","M","kW","0.018"]
["","","","L","kW","0.012"]
["","","","Klusums","kW","0.011"]
["","Ūdens tvertnes tilpums","","","l","3.6"]
["Skaņas spiediena līmenis","Gaisa attīrīšanas darbība","","Turbo","dBA","54"]
["","","","Vidēja","dBA","37"]
["","","","Zema","dBA","27"]
["","","","Klusums","dBA","18"]
["","Mitrināšanas darbība","","Turbo","dBA","54"]
["","","","Vidēja","dBA","37"]
["","","","Zema","dBA","27"]
["","","","Klusums","dBA","23"]
["Ventilators","Gaisa plūsmas ātrums","Gaisa attīrīšanas darbība","Turbo","m³/h","420"]
["","","","Vidēja","m³/h","210"]
["","","","Zema","m³/h","132"]
["","","","Klusums","m³/h","60"]
["","","Mitrināšanas darbība","Turbo","m³/h","420"]
["","","","Vidēja","m³/h","210"]
["","","","Zema","m³/h","132"]
["","","","Klusums","m³/h","102"]
["Putekļu savākšanas metode","","","","","Elektrostatiskais HEPA filtrs"]
["Dezodorēšanas metode","","","","","Flash streamer + dezodorējošais katalizators"]
["Standard Accessories","Operation manual","","","","1"]
["","Electrostatic HEPA filter","","","","1"]
["","Deodorising filter","","","","1"]
["","Caster","","","","4"]
["","Humidifying filter","","","","1"]
["Barošanas vads","m","","","","2"]
["Barošanas avots","Fāze","","","","1~"]
["Strāvas padeve","Frekvence","","","Hz","50/60"]
["","Spriegums","","","V","220-240/220-230"]
["Notes","","","","","(1) - Aptveršanas zona ir atbilstoša iekārtas darbināšanai ar maksimālu ventilatora ātrumu (HH). Aptveršanas zona norāda platību, kurā noteiktu putekļu daļiņu daudzumu var likvidēt 30 minūšu laikā."]
["","","","","","(2) - Konvertēts uz NRCC standartiem no testu vērtībām saskaņā ar JEM1467."]
["","","","","","(3) - Darbības skaņas līmeņi ir to vērtību vidējā vērtība, kas mērīti 1 m atstatumā no ierīces priekšpuses, kreisās puses, labās puses un augšas. (Tā ir vienāda ar vērtību bezatbalss nodalījumā)"]