{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":35,"n_cols":6,"rows_kept":35,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXLG-M"]
[]
[]
[]
[]
["","","","","","RXLG25M2V1B"]
["Ventilators","Gaisa plūsmas ātrums","Dzesēšana","Sevišķi lēns","m³/min.","30.6"]
["","","Apsilde","Sevišķi lēns","m³/min.","27.2"]
["","","","Sevišķi lēns","cfm","1080"]
["","","Apsilde","Sevišķi lēns","cfm","960"]
["Izmēri","Ierīce","","Augstums","mm","550"]
["","","","Platums","mm","858"]
["","","","Dziļums","mm","330"]
["Svars","Ierīce","","","kg","40"]
["Kompresors","Veids","","","","Hermētiski noblīvēts šūpojošais kompresors"]
["Darbības amplitūda","Dzesēšana","Apkārtējā vide","Min.","°CDB","-10"]
["","","","Maks.","°CDB","46"]
["","Apsilde","Apkārtējā vide","Min.","° CWB","-25"]
["","","","Maks.","° CWB","18"]
["Skaņas spiediena līmenis","Dzesēšana","","Augsta","dBA","48"]
["","","","Zema","dBA","44"]
["","Apsilde","","Augsta","dBA","49"]
["","","","Zema","dBA","45"]
["Aukstumaģents","Tips","","","","R-410A"]
["","Daudzums","","","kg","1"]
["","Daudzums","","","tCO2Eq","2.1"]
["","GWP","","","","2087.5"]
["Cauruļvadu savienojumi","Cauruļvadu garums","Maks.","Ārējā ierīce — iekštelpu ierīce","m","20"]
["","Papildu dzesētāja uzlāde","","","kg/m","0,02 (cauruļvadu garumam, kas pārsniedz 10 m)"]
["","Līmeņa atšķirība","Iekštelpu ierīce-iekštelpu ierīce","Maks.","m","15"]
["Standard Accessories","Installation manual","","","","1"]
["","Drain plug","","","","1"]
["Barošanas avots","Fāze","","","","1~"]
["Strāvas padeve","Frekvence","","","Hz","50"]
["","Spriegums","","","V","220-240"]