{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":56,"n_cols":11,"rows_kept":56,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-F"]
[]
[]
[]
[]
["","","","","","RXS60F4V1B","RXS60F2V1B","RXS60F3V1B","RXS71FAV1B9","RXS71FV1B","RXS71FAV1B"]
["Skaņas spiediena līmenis","Apsilde","","Augsta","dBA","49","","","52"]
["","","","Zema","dBA","46","","","49"]
["","Dzesēšana","","Zema","dBA","46","","","49"]
["","","","Augsta","dBA","49","","","52"]
["Standard Accessories","Izplūdes ligzda","","","","1","","","1"]
["","Uzstādīšanas rokasgrāmata","","","","1","","","1"]
["Aukstumaģents","Charge","","","TCO2Eq","3.1","","","4.8"]
["","GWP","","","","2,087.5","","","2,087.5"]
["","Charge","","","kg","1.5","","","2.3"]
["","Tips","","","","R-410A","","","R-410A"]
["Cauruļu savienojumi","Līmeņa atšķirība","Iekštelpu ierīce – āra ierīce","Maks.","m","20","","","20"]
["","Papildu dzesētāja uzlāde","","","kg/m","0,02 (cauruļvadu garumam, kas pārsniedz 10 m)","","","0,02 (cauruļvadu garumam, kas pārsniedz 10 m)"]
["Kompresors","Veids","","","","Hermētiski noblīvēts šūpojošais kompresors","","","Hermētiski noblīvēts šūpojošais kompresors"]
["Izmēri","Ierīce","","Platums","mm","825","","","900"]
["","","","Dziļums","mm","300","","","320"]
["","","","Augstums","mm","735","","","770"]
["Svars","Ierīce","","","kg","48","","","71"]
["Power supply","Fāze","","","","1~","","","1~"]
["","Frekvence","","","Hz","50","","","50"]
["","Spriegums","","","V","220-240","","","220-240"]
["Notes","","","","","(1) - SL: gaisa plūsmas ātruma iestatījuma klusais ventilatora līmenis","(1) - 220 V","","(1) - SL: gaisa plūsmas ātruma iestatījuma klusais ventilatora līmenis","(1) - 220 V"]
["","","","","","(2) - Satur fluorētas siltumnīcefekta gāzes","(2) - 230 V","","(2) - Satur fluorētas siltumnīcefekta gāzes","(2) - 230 V"]
["Izmēri","Ierīce","","Augstums","mm","","735","735","","770","770"]
["","","","Platums","mm","","825","825","","900","900"]
["","","","Dziļums","mm","","300","300","","320","320"]
["Svars","Ierīce","","","kg","","48","48","","71","71"]
["Kompresors","Veids","","","","","Hermētiski noblīvēts šūpojošais kompresors","Hermētiski noblīvēts šūpojošais kompresors","","Hermētiski noblīvēts šūpojošais kompresors","Hermētiski noblīvēts šūpojošais kompresors"]
["Darbības amplitūda","Dzesēšana","Apkārtējā vide","Min.","°CDB","","-10","-10","","-10","-10"]
["","","","Maks.","°CDB","","46","46","","46","46"]
["","Apsilde","Apkārtējā vide","Min.","° CWB","","-15","-15","","-15","-15"]
["","","","Maks.","° CWB","","18","20","","18","20"]
["Skaņas spiediena līmenis","Dzesēšana","","Augsta","dBA","","49","49","","52","52"]
["","","","Zema","dBA","","46","46","","49","49"]
["","Apsilde","","Augsta","dBA","","49","49","","52","52"]
["","","","Zema","dBA","","46","46","","49","49"]
["Aukstumaģents","Tips","","","","","R-410A","R-410A","","R-410A","R-410A"]
["","Daudzums","","","kg","","1.5","1.5","","2.3","2.3"]
["","Daudzums","","","tCO2Eq","","3.1","3.1","","4.8","4.8"]
["","GWP","","","","","2087.5","2087.5","","2087.5","2087.5"]
["Cauruļvadu savienojumi","Cauruļvadu garums","Maks.","Ārējā ierīce — iekštelpu ierīce","m","","30","30","","30","30"]
["","Papildu dzesētāja uzlāde","","","kg/m","","0,02 (cauruļvadu garumam, kas pārsniedz 10 m)","0,02 (cauruļvadu garumam, kas pārsniedz 10 m)","","0,02 (cauruļvadu garumam, kas pārsniedz 10 m)","0,02 (cauruļvadu garumam, kas pārsniedz 10 m)"]
["","Līmeņa atšķirība","Iekštelpu ierīce – āra ierīce","Maks.","m","","20","20","","20","20"]
["Standard Accessories","Installation manual","","","","","Installation manual","1","","Installation manual","1"]
["","Drain plug","","","","","Drain plug","","","Drain plug"]
["Barošanas avots","Fāze","","","","","1~","1~","","1~","1~"]
["Strāvas padeve","Frekvence","","","Hz","","50","50","","50","50"]
["","Spriegums","","","V","","220-240","220-240","","220-240","220-240"]
["Notes","","","","","","(3) - 240 V","","","(3) - 240 V"]
["Standard Accessories","Drain socket","","","","","","1","","","1"]
["Sound power level","Dzesēšana","","","dBA","","","","65"]