{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":59,"n_cols":12,"rows_kept":59,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-K"]
[]
[]
[]
[]
["","","","","","RXS20K3V1B","RXS20K2V1B","RXS25K3V1B","RXS25K2V1B","RXS35K2V1B","RXS42K2V1B","RXS50K2V1B"]
["Skaņas spiediena līmenis","Apsilde","","Augsta","dBA","47","","47","","48","48","48"]
["","Dzesēšana","","Augsta","dBA","46","","46","","48","48","48"]
["Standard Accessories","Izplūdes aizbāznis","","","","","","","","1","1","1"]
["","Uzstādīšanas rokasgrāmata","","","","1","","1","","1","1","1"]
["Refrigerant","Charge","","","TCO2Eq","2.1","","2.1","","2.5","2.7","3.5"]
["","GWP","","","","2,087.5","","2,087.5","","2,087.5","2,087.5","2,087.5"]
["","Uzlāde","","","kg","1.0","","1.0","","1.2","1.3","1.7"]
["","Tips","","","","R-410A","","R-410A","","R-410A","R-410A","R-410A"]
["Ventilatora motors","Ātrums","Dzesēšana","Sevišķi lēns","apgr./min.","780","","780","","780","790","670"]
["","","Apsilde","Sevišķi lēns","apgr./min.","740","","740","","740","780","670"]
["Cauruļu savienojumi","Līmeņa atšķirība","Iekštelpu ierīce – āra ierīce","Maks.","m","15","","15","","15","15","20"]
["","Papildu dzesētāja uzlāde","","","kg/m","0,02 (cauruļvadu garumam, kas pārsniedz 10 m)","","0,02 (cauruļvadu garumam, kas pārsniedz 10 m)","","0,02 (cauruļvadu garumam, kas pārsniedz 10 m)","0,02 (cauruļvadu garumam, kas pārsniedz 10 m)","0,02 (cauruļvadu garumam, kas pārsniedz 10 m)"]
["Kompresors","Veids","","","","Hermētiski noblīvēts šūpojošais kompresors","","Hermētiski noblīvēts šūpojošais kompresors","","Hermētiski noblīvēts šūpojošais kompresors","Hermētiski noblīvēts šūpojošais kompresors","Hermētiski noblīvēts šūpojošais kompresors"]
["Izmēri","Ierīce","","Platums","mm","765","","765","","765","765","825"]
["","","","Dziļums","mm","285","","285","","285","285","300"]
["","","","Augstums","mm","550","","550","","550","550","735"]
["Svars","Ierīce","","","kg","34","","34","","34","39","47"]
["Ventilators","Gaisa plūsmas ātrums","Apsilde","Sevišķi lēns","cfm","","","","","904","960","1,522"]
["","","Dzesēšana","Sevišķi lēns","cfm","","","","","1,063","1,080","1,727"]
["Power supply","Fāze","","","","1~","","1~","","1~","1~","1~"]
["","Frekvence","","","Hz","50","","50","","50","50","50"]
["","Spriegums","","","V","220-240","","220-240","","220-240","220-240","220-240"]
["Notes","","","","","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V"]
["","","","","","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V"]
["","","","","","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V"]
["","","","","","(4) - SL: gaisa plūsmas ātruma iestatījuma klusais ventilatora līmenis","","(4) - SL: gaisa plūsmas ātruma iestatījuma klusais ventilatora līmenis","","(4) - Satur fluorētas siltumnīcefekta gāzes","(4) - Satur fluorētas siltumnīcefekta gāzes","(4) - Satur fluorētas siltumnīcefekta gāzes"]
["Standard Accessories","Savienojums (novadcaurule)","","","","1","","1"]
["Notes","","","","","(5) - Satur fluorētas siltumnīcefekta gāzes","","(5) - Satur fluorētas siltumnīcefekta gāzes"]
["Izmēri","Ierīce","","Augstums","mm","","550","","550"]
["","","","Platums","mm","","765","","765"]
["","","","Dziļums","mm","","285","","285"]
["Svars","Ierīce","","","kg","","34","","34"]
["Ventilatora motors","Ātrums","Dzesēšana","Sevišķi lēns","apgr./min.","","780","","780"]
["","","Apsilde","Sevišķi lēns","apgr./min.","","740","","740"]
["Kompresors","Veids","","","","","Hermētiski noblīvēts šūpojošais kompresors","","Hermētiski noblīvēts šūpojošais kompresors"]
["Darbības amplitūda","Dzesēšana","Apkārtējā vide","Min.","°CDB","","-10","","-10"]
["","","","Maks.","°CDB","","46","","46"]
["","Apsilde","Apkārtējā vide","Min.","° CWB","","-15","","-15"]
["","","","Maks.","° CWB","","18","","18"]
["Skaņas spiediena līmenis","Dzesēšana","","Augsta","dBA","","46","","46"]
["","Apsilde","","Augsta","dBA","","47","","47"]
["Aukstumaģents","Tips","","","","","R-410A","","R-410A"]
["","Daudzums","","","kg","","1.0","","1.0"]
["","Daudzums","","","tCO2Eq","","2.1","","2.1"]
["","GWP","","","","","2087.5","","2087.5"]
["Cauruļvadu savienojumi","Cauruļvadu garums","Maks.","Ārējā ierīce — iekštelpu ierīce","m","","20","","20"]
["","Papildu dzesētāja uzlāde","","","kg/m","","0,02 (cauruļvadu garumam, kas pārsniedz 10 m)","","0,02 (cauruļvadu garumam, kas pārsniedz 10 m)"]
["","Līmeņa atšķirība","Iekštelpu ierīce – āra ierīce","Maks.","m","","15","","15"]
["Standard Accessories","Installation manual","","","","","1","","1"]
["","Joint (drain)","","","","","1","","1"]
["Barošanas avots","Fāze","","","","","1~","","1~"]
["Strāvas padeve","Frekvence","","","Hz","","50","","50"]
["","Spriegums","","","V","","220-240","","220-240"]