{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":72,"n_cols":8,"rows_kept":72,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-L3"]
[]
[]
[]
[]
["","","","","","RXS20L3V1B","RXS25L3V1B","RXS35L3V1B"]
["Skaņas spiediena līmenis","Apsilde","","Augsta","dBA","","","48"]
["","Dzesēšana","","Augsta","dBA","","","48"]
["Standard Accessories","Uzstādīšanas rokasgrāmata","","","","","","1"]
["","Dzesētāja padeves marķējums","","","","","","1"]
["","Vairākvalodu fluorinēto siltumnīcu gāzu marķējumi","","","","","","1"]
["","Drenāžas aizbāznis (tikai siltumsūkņa modeļiem)","","","","","","1"]
["Aukstumaģents","Charge","","","TCO2Eq","","","2.5"]
["","GWP","","","","","","2,087.5"]
["","Charge","","","kg","","","1.2"]
["","Tips","","","","","","R-410A"]
["Ventilatora motors","Ātrums","Dzesēšana","Sevišķi lēns","apgr./min.","","","780"]
["","","Apsilde","Sevišķi lēns","apgr./min.","","","740"]
["Darbības amplitūda","Dzesēšana","Apkārtējā vide","Maks.","°CDB","","","46"]
["","","","Min.","°CDB","","","-10"]
["","Apsilde","Apkārtējā vide","Maks.","° CWB","","","18"]
["","","","Min.","° CWB","","","-15"]
["Cauruļu savienojumi","Līmeņa atšķirība","Iekštelpu ierīce – āra ierīce","Maks.","m","","","15"]
["","Papildu dzesētāja uzlāde","","","kg/m","","","0,02 (cauruļvadu garumam, kas pārsniedz 10 m)"]
["Kompresors","Veids","","","","","","Hermētiski noblīvēts šūpojošais kompresors"]
["Izmēri","Ierīce","","Platums","mm","","","765"]
["","","","Dziļums","mm","","","285"]
["","","","Augstums","mm","","","550"]
["Svars","Ierīce","","","kg","","","34"]
["Ventilators","Gaisa plūsmas ātrums","Apsilde","Sevišķi lēns","cfm","","","904"]
["","","","Sevišķi lēns","m³/min.","","","25.6"]
["","","Dzesēšana","Sevišķi lēns","m³/min.","","","30.1"]
["","","","Sevišķi lēns","cfm","","","1,063"]
["Power supply","Fāze","","","","","","1~"]
["","Frekvence","","","Hz","","","50"]
["","Spriegums","","","V","","","220-240"]
["Notes","","","","","","","(1) - SL: gaisa plūsmas ātruma iestatījuma klusais ventilatora līmenis"]
["Ventilators","Gaisa plūsmas ātrums","Dzesēšana","Sevišķi lēns","m³/min.","30.1","30.1"]
["","","Apsilde","Sevišķi lēns","m³/min.","25.6","25.6"]
["","","","Sevišķi lēns","cfm","1063","1063"]
["","","Apsilde","Sevišķi lēns","cfm","904","904"]
["Izmēri","Ierīce","","Augstums","mm","550","550"]
["","","","Platums","mm","765","765"]
["","","","Dziļums","mm","285","285"]
["Svars","Ierīce","","","kg","34","34"]
["Ventilatora motors","Ātrums","Dzesēšana","Sevišķi lēns","apgr./min.","780","780"]
["","","Apsilde","Sevišķi lēns","apgr./min.","740","740"]
["Kompresors","Veids","","","","Hermētiski noblīvēts šūpojošais kompresors","Hermētiski noblīvēts šūpojošais kompresors"]
["Darbības amplitūda","Dzesēšana","Apkārtējā vide","Min.","°CDB","-10","-10"]
["","","","Maks.","°CDB","46","46"]
["","Apsilde","Apkārtējā vide","Min.","° CWB","-15","-15"]
["","","","Maks.","° CWB","18","18"]
["Skaņas spiediena līmenis","Dzesēšana","","Augsta","dBA","46","46"]
["","Apsilde","","Augsta","dBA","47","47"]
["Aukstumaģents","Tips","","","","R-410A","R-410A"]
["","Daudzums","","","kg","1.0","1.0"]
["","Daudzums","","","tCO2Eq","2.1","2.1"]
["","GWP","","","","2087.5","2087.5"]
["Cauruļvadu savienojumi","Cauruļvadu garums","Maks.","Ārējā ierīce — iekštelpu ierīce","m","20","20"]
["","Papildu dzesētāja uzlāde","","","kg/m","0,02 (cauruļvadu garumam, kas pārsniedz 10 m)","0,02 (cauruļvadu garumam, kas pārsniedz 10 m)"]
["","Līmeņa atšķirība","Iekštelpu ierīce – āra ierīce","Maks.","m","15","15"]
["Standard Accessories","Installation manual","","","","1","1"]
["","Refrigerant charge label","","","","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1"]
["","Drain plug","","","","1"]
["Barošanas avots","Fāze","","","","1~","1~"]
["Strāvas padeve","Frekvence","","","Hz","50","50"]
["","Spriegums","","","V","220-240","220-240"]
["Notes","","","","","(1) - 220 V"]
["","","","","","(2) - 230 V"]
["","","","","","(3) - 240 V"]
["Standard Accessories","Drain plug (only heat pump models)","","","","","1"]