{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":6,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXTA-B"]
[]
[]
[]
[]
["","","","","","RXTA30B2V1B"]
["Izmēri","Ierīce","","Augstums","mm","551"]
["","","","Platums","mm","763"]
["","","","Dziļums","mm","312"]
["Svars","Ierīce","","","kg","38"]
["Ventilatora motors","Ātrums","Dzesēšana","Sevišķi lēns","apgr./min.","450"]
["","","Apsilde","Sevišķi lēns","apgr./min.","360"]
["Kompresors","Veids","","","","Hermētiski noblīvēts šūpojošais kompresors"]
["Darbības amplitūda","Dzesēšana","Apkārtējā vide","Min.","°CDB","-10"]
["","","","Maks.","°CDB","46"]
["","Apsilde","Apkārtējā vide","Min.","° CWB","-25"]
["","","","Maks.","° CWB","18"]
["Skaņas spiediena līmenis","Dzesēšana","","Nom.","dBA","48"]
["","Apsilde","","Nom.","dBA","49"]
["Aukstumaģents","Tips","","","","R-32"]
["","Daudzums","","","kg","1.1"]
["","Daudzums","","","tCO2Eq","0.74"]
["","GWP","","","","675"]
["Cauruļvadu savienojumi","Cauruļvadu garums","Maks.","Ārējā ierīce — iekštelpu ierīce","m","20"]
["","Papildu dzesētāja uzlāde","","","kg/m","0,02 (cauruļvadu garumam, kas pārsniedz 10 m)"]
["","Līmeņa atšķirība","Iekštelpu ierīce – āra ierīce","Maks.","m","15"]
["Standard Accessories","Uzstādīšanas rokasgrāmata","","","","1"]
["","Dzesētāja padeves marķējums","","","","1"]
["","Vairākvalodu fluorinēto siltumnīcu gāzu marķējumi","","","","1"]
["Energoefektivitātes diapazons","","","","","A+++ ~ D"]
["Barošanas avots","Fāze","","","","1~"]
["Strāvas padeve","Frekvence","","","Hz","50"]
["","Spriegums","","","V","220-240"]
["Notes","","","","","(1) - Satur fluorētas siltumnīcefekta gāzes"]
["","","","","","(2) - Darbības diapazonu skatiet atsevišķā attēlā"]
["","","","","","(3) - Elektrības datus skatiet atsevišķā zīmējumā"]