{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":7,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXTM-N"]
[]
[]
[]
[]
["","","","","","RXTM30N2V1B","RXTM40N2V1B"]
["Skaņas spiediena līmenis","Apsilde","","Nom.","dBA","49","49"]
["","Dzesēšana","","Nom.","dBA","48","48"]
["Standard Accessories","Uzstādīšanas rokasgrāmata","","","","1","1"]
["","Dzesētāja padeves marķējums","","","","1","1"]
["","Vairākvalodu fluorinēto siltumnīcu gāzu marķējumi","","","","1","1"]
["Refrigerant","Charge","","","TCO2Eq","0.7","0.7"]
["","GWP","","","","675","675"]
["","Uzlāde","","","kg","1.1","1.1"]
["","Tips","","","","R-32","R-32"]
["Ventilatora motors","Ātrums","Dzesēšana","Sevišķi lēns","apgr./min.","450","360"]
["","","Apsilde","Sevišķi lēns","apgr./min.","360","360"]
["Cauruļu savienojumi","Līmeņa atšķirība","Iekštelpu ierīce – āra ierīce","Maks.","m","15","15"]
["","Papildu dzesētāja uzlāde","","","kg/m","0,02 (cauruļvadu garumam, kas pārsniedz 10 m)","0,02 (cauruļvadu garumam, kas pārsniedz 10 m)"]
["Kompresors","Veids","","","","Hermētiski noblīvēts šūpojošais kompresors","Hermētiski noblīvēts šūpojošais kompresors"]
["Izmēri","Ierīce","","Platums","mm","763","763"]
["","","","Dziļums","mm","312","312"]
["","","","Augstums","mm","551","551"]
["Svars","Ierīce","","","kg","38","38"]
["Power supply","Fāze","","","","1~","1~"]
["","Frekvence","","","Hz","50","50"]
["","Spriegums","","","V","220-240","220-240"]
["Notes","","","","","(1) - Satur fluorētas siltumnīcefekta gāzes","(1) - Satur fluorētas siltumnīcefekta gāzes"]
["","","","","","(2) - Darbības diapazonu skatiet atsevišķā attēlā","(2) - Darbības diapazonu skatiet atsevišķā attēlā"]
["","","","","","(3) - Elektrības datus skatiet atsevišķā zīmējumā","(3) - Elektrības datus skatiet atsevišķā zīmējumā"]