{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":7,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXTP-A"]
[]
[]
[]
[]
["","","","","","RXTP25A2V1B","RXTP35A2V1B"]
["Izmēri","Ierīce","","Augstums","mm","605","605"]
["","","","Platums","mm","930","930"]
["","","","Dziļums","mm","376","376"]
["Svars","Ierīce","","","kg","42","42"]
["Ventilatora motors","Ātrums","Dzesēšana","Sevišķi lēns","apgr./min.","800","800"]
["","","Apsilde","Sevišķi lēns","apgr./min.","400","400"]
["Kompresors","Veids","","","","Hermētiski noblīvēts šūpojošais kompresors","Hermētiski noblīvēts šūpojošais kompresors"]
["Darbības amplitūda","Dzesēšana","Apkārtējā vide","Min.","°CDB","-10","-10"]
["","","","Maks.","°CDB","46","46"]
["","Apsilde","Apkārtējā vide","Min.","° CWB","-31","-31"]
["","","","Maks.","° CWB","18","18"]
["Skaņas spiediena līmenis","Dzesēšana","","Nom.","dBA","48","48"]
["","Apsilde","","Nom.","dBA","49.0","49.0"]
["Aukstumaģents","Tips","","","","R-32","R-32"]
["","Daudzums","","","kg","0.97","0.97"]
["","Daudzums","","","tCO2Eq","0.66","0.66"]
["","GWP","","","","675.0","675.0"]
["Cauruļvadu savienojumi","Cauruļvadu garums","Maks.","Ārējā ierīce — iekštelpu ierīce","m","20","20"]
["","Papildu dzesētāja uzlāde","","","kg/m","0,02 (cauruļvadu garumam, kas pārsniedz 10 m)","0,02 (cauruļvadu garumam, kas pārsniedz 10 m)"]
["","Līmeņa atšķirība","Iekštelpu ierīce – āra ierīce","Maks.","m","15.0","15.0"]
["Standard Accessories","Installation manual","","","","1","1"]
["","Refrigerant charge label","","","","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1"]
["Barošanas avots","Fāze","","","","1~","1~"]
["Strāvas padeve","Frekvence","","","Hz","50","50"]
["","Spriegums","","","V","220-240","220-240"]