{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":52,"n_cols":11,"rows_kept":52,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXZ-N"]
[]
[]
[]
[]
["","","","","","RXZ25NV1B","RXZ25NV1B9","RXZ35NV1B","RXZ35NV1B9","RXZ50NV1B","RXZ50NV1B9"]
["Skaņas spiediena līmenis","Apsilde","","Augsta","dBA","","","48","48","50","50"]
["","Dzesēšana","","Augsta","dBA","","","48","48","49","49"]
["Standard Accessories","Lietošanas rokasgrāmata","","","","","","1","1","1","1"]
["","Uzstādīšanas rokasgrāmata","","","","","","1","1","1","1"]
["Aukstumaģents","GWP","","","","","","675","675","675","675"]
["","Charge","","","kg","","","1.34","1.34","1.34","1.34"]
["","Tips","","","","","","R-32","R-32","R-32","R-32"]
["Darbības amplitūda","Dzesēšana","Apkārtējā vide","Maks.","°CDB","","","43","43","43","43"]
["","","","Min.","°CDB","","","-10","-10","-10","-10"]
["","Apsilde","Apkārtējā vide","Maks.","° CWB","","","18","18","18","18"]
["","","","Min.","° CWB","","","-20","-20","-20","-20"]
["Cauruļu savienojumi","Līmeņa atšķirība","Iekštelpu ierīce – āra ierīce","Maks.","m","","","8","8","8","8"]
["Izmēri","Ierīce","","Platums","mm","","","795","795","795","795"]
["","","","Dziļums","mm","","","300","300","300","300"]
["","","","Augstums","mm","","","693","693","693","693"]
["Kompresors","Veids","","","","","","Hermētiski noblīvēts šūpojošais kompresors","Hermētiski noblīvēts šūpojošais kompresors","Hermētiski noblīvēts šūpojošais kompresors","Hermētiski noblīvēts šūpojošais kompresors"]
["Svars","Ierīce","","","kg","","","50","50","50","50"]
["Power supply","Fāze","","","","","","1~","1~","1~","1~"]
["","Frekvence","","","Hz","","","50","50","50","50"]
["","Spriegums","","","V","","","220-240","220-240","220-240","220-240"]
["Notes","","","","","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V"]
["","","","","","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V"]
["","","","","","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V"]
["","","","","","","","(4) - Satur fluorētas siltumnīcefekta gāzes","(4) - Satur fluorētas siltumnīcefekta gāzes","(4) - Satur fluorētas siltumnīcefekta gāzes","(4) - Satur fluorētas siltumnīcefekta gāzes"]
["Izmēri","Ierīce","","Augstums","mm","693","693"]
["","","","Platums","mm","795","795"]
["","","","Dziļums","mm","300","300"]
["Svars","Ierīce","","","kg","50","50"]
["Kompresors","Veids","","","","Hermētiski noblīvēts šūpojošais kompresors","Hermētiski noblīvēts šūpojošais kompresors"]
["Darbības amplitūda","Dzesēšana","Apkārtējā vide","Min.","°CDB","-10","-10"]
["","","","Maks.","°CDB","43","43"]
["","Apsilde","Apkārtējā vide","Min.","° CWB","-20","-20"]
["","","","Maks.","° CWB","18","18"]
["Skaņas spiediena līmenis","Dzesēšana","","Augsta","dBA","46","46"]
["","Apsilde","","Augsta","dBA","46","46"]
["Aukstumaģents","Tips","","","","R-32","R-32"]
["","Daudzums","","","kg","1.34","1.34"]
["","Daudzums","","","tCO2Eq","0.9","0.9"]
["","GWP","","","","675","675"]
["Cauruļvadu savienojumi","Cauruļvadu garums","Maks.","Ārējā ierīce — iekštelpu ierīce","m","10","10"]
["","Līmeņa atšķirība","Iekštelpu ierīce – āra ierīce","Maks.","m","8","8"]
["Standard Accessories","Installation manual","","","","1","1"]
["","Operation manual","","","","1","1"]
["Barošanas avots","Fāze","","","","1~","1~"]
["Strāvas padeve","Frekvence","","","Hz","50","50"]
["","Spriegums","","","V","220-240","220-240"]