{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":7,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZA-D"]
[]
[]
[]
[]
["","","","","","RZA200D7Y1B","RZA250D7Y1B"]
["Izmēri","Ierīce","","Augstums","mm","870","870"]
["","","","Platums","mm","1,100","1,100"]
["","","","Dziļums","mm","460","460"]
["Svars","Ierīce","","","kg","117","117"]
["Kompresors","Type","","","","Hermētiski noblīvēts spirālveida kompresors","Hermētiski noblīvēts spirālveida kompresors"]
["Darbības diapazons","Dzesēšana","Apkārtējā vide","Min.","°CDB","-20","-20"]
["","","","Maks.","°CDB","46","46"]
["","Apsilde","Apkārtējā vide","Min.","° CWB","-20","-20"]
["","","","Maks.","° CWB","15","15"]
["Skaņas jaudas līmenis","Dzesēšana","","","dBA","73","76"]
["","Apsilde","","","dBA","76 (1)","79 (1)"]
["Skaņas spiediena līmenis","Dzesēšana","","Nom.","dBA","53","57"]
["","Apsilde","","Nom.","dBA","60","63"]
["Aukstumaģents","Tips","","","","R-32","R-32"]
["","Daudzums","","","kg","5","5"]
["","GWP","","","","675","675"]
["Piping connections","Šķidrums","","OD","mm","9.52","9.52"]
["","Gāze","","OD","mm","22.2","22.2"]
["","Cauruļvadu garums","Maks.","Ārējā ierīce — iekštelpu ierīce","m","100","100"]
["","","Sistēma","Neuzlādēts","m","30","30"]
["","Papildu dzesētāja uzlāde","","","kg/m","Skatiet uzstādīšanas rokasgrāmatu","Skatiet uzstādīšanas rokasgrāmatu"]
["Standard Accessories","Uzstādīšanas rokasgrāmata","","","","1","1"]
["","Vispārēji drošības pasākumi","","","","1","1"]
["","Sasienamie iesaiņojumi","","","","2","2"]
["","Noņemama F-gas uzlīme","","","","1","1"]
["","Savienojuma cauruļvadi","","","","6","6"]
["Power supply","Phase","","","","3~","3~"]
["","Frekvence","","","Hz","50","50"]
["","Spriegums","","","V","380-415","380-415"]
["Strāva - 50 Hz","Maks. drošinātāja ampēri (MFA)","","","A","20","20"]
["Notes","","","","","(1) - Saskaņā ar ENER Lot 21","(1) - Saskaņā ar ENER Lot 21"]