{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":35,"n_cols":8,"rows_kept":35,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZAG-A"]
[]
[]
[]
[]
["","","","","","RZAG35A2V1B","RZAG50A2V1B","RZAG60A2V1B"]
["Izmēri","Ierīce","","Augstums","mm","734","734","734"]
["","","","Platums","mm","870","870","870"]
["","","","Dziļums","mm","373","373","373"]
["Svars","Ierīce","","","kg","52","52","52"]
["Kompresors","Veids","","","","Hermētiski noblīvēts šūpojošais kompresors","Hermētiski noblīvēts šūpojošais kompresors","Hermētiski noblīvēts šūpojošais kompresors"]
["Skaņas jaudas līmenis","Dzesēšana","","","dBA","62.0","63.0","64.0"]
["","Apsilde","","","dBA","62.0","63.0","64.0"]
["Skaņas spiediena līmenis","Dzesēšana","","Nom.","dBA","48.0","49.0","50.0"]
["","Apsilde","","Nom.","dBA","48.0","49.0","50.0"]
["Aukstumaģents","Tips","","","","","R-32"]
["","Daudzums","","","kg","1.55","1.55","1.55"]
["","GWP","","","","675.0","675.0","675.0"]
["","Daudzums","","","tCO2Eq","1.05","1.05","1.05"]
["Cauruļu savienojumi","Šķidrums","","OD","mm","6.35","6.35","6.35"]
["","Gāze","","OD","mm","9.50","12.7","12.7"]
["Cauruļvadu savienojumi","Cauruļvadu garums","Maks.","Ārējā ierīce — iekštelpu ierīce","m","50","50","50"]
["","","Sistēma","Neuzlādēts","m","30","30","30"]
["","Papildu dzesētāja uzlāde","","","kg/m","0,02 (cauruļvadu garumam, kas pārsniedz 30 m)","0,02 (cauruļvadu garumam, kas pārsniedz 30 m)","0,02 (cauruļvadu garumam, kas pārsniedz 30 m)"]
["","Līmeņa atšķirība","Iekštelpu ierīce – āra ierīce","Maks.","m","30.0","30.0","30.0"]
["Standard Accessories","Installation manual","","","","1","1","1"]
["","Refrigerant charge label","","","","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1"]
["","General safety precautions","","","","1","1","1"]
["","LOT10 Energy Label","","","","1","1","1"]
["","Drain cap","","","","3","3","3"]
["","Drain plug","","","","1","1","1"]
["Barošanas avots","Fāze","","","","","1~"]
["Strāvas padeve","Frekvence","","","Hz","50","50","50"]
["","Spriegums","","","V","","220-240"]