{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":13,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZAG-NV1"]
[]
[]
[]
[]
["","","","","","RZAG71N7V1B","RZAG71N2V1B","RZAG100N7V1B","RZAG100N2V1B","RZAG125N7V1B","RZAG125N2V1B","RZAG140N7V1B","RZAG140N2V1B"]
["Izmēri","Ierīce","","Augstums","mm","870","870","870","870","870","870","870","870"]
["","","","Platums","mm","1100","1100","1100","1100","1100","1100","1100","1100"]
["","","","Dziļums","mm","460","460","460","460","460","460","460","460"]
["Svars","Ierīce","","","kg","81","81","85","85","95","95","95","95"]
["Kompresors","Type","","","","","","Hermētiski noblīvēts šūpojošais kompresors","Hermētiski noblīvēts šūpojošais kompresors","Hermētiski noblīvēts šūpojošais kompresors","Hermētiski noblīvēts šūpojošais kompresors","Hermētiski noblīvēts šūpojošais kompresors","Hermētiski noblīvēts šūpojošais kompresors"]
["Darbības amplitūda","Dzesēšana","Apkārtējā vide","Min.","°CDB","-20","-20","-20","-20","-20","-20","-20","-20"]
["","","","Maks.","°CDB","52","52","52","52","52","52","52","52"]
["","Apsilde","Apkārtējā vide","Min.","° CWB","-20","-20","-20","-20","-20","-20","-20","-20"]
["","","","Maks.","° CWB","18","18","18","18","18","18","18","18"]
["Skaņas jaudas līmenis","Dzesēšana","","","dBA","64","64","66","66","69","69","70","70"]
["","Apsilde","","","dBA","","","","","68 (1)","68 (1)","71 (1)","71 (1)"]
["Skaņas spiediena līmenis","Dzesēšana","","Nom.","dBA","46","46","47","47","49","49","50","50"]
["","Apsilde","","Nom.","dBA","48","48","50","50","52","52","52","52"]
["Aukstumaģents","Tips","","","","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32"]
["","Daudzums","","","kg","3.2","3.20","3.2","3.20","3.7","3.70","3.7","3.70"]
["","GWP","","","","675","675","675","675","675","675","675","675"]
["","Daudzums","","","tCO2Eq","2.16","2.16","2.16","2.16","2.5","2.50","2.5","2.50"]
["Cauruļu savienojumi","Šķidrums","","OD","mm","10","10","10","10","10","10","10","10"]
["","Gāze","","OD","mm","15.9","15.9","15.9","15.9","15.9","15.9","15.9","15.9"]
["Cauruļvadu savienojumi","Cauruļvadu garums","Maks.","Ārējā ierīce — iekštelpu ierīce","m","55","55","85","85","85","85","85","85"]
["","","Sistēma","Ekvivalents","m","75","75","100","100","100","100","100","100"]
["","","","Neuzlādēts","m","40","40","40","40","40","40","40","40"]
["","Papildu dzesētāja uzlāde","","","kg/m","Skatiet uzstādīšanas rokasgrāmatu","Skatiet uzstādīšanas rokasgrāmatu","Skatiet uzstādīšanas rokasgrāmatu","Skatiet uzstādīšanas rokasgrāmatu","Skatiet uzstādīšanas rokasgrāmatu","Skatiet uzstādīšanas rokasgrāmatu","Skatiet uzstādīšanas rokasgrāmatu","Skatiet uzstādīšanas rokasgrāmatu"]
["","Līmeņa atšķirība","Iekštelpu ierīce – āra ierīce","Maks.","m","30","30","30","30","30","30","30","30"]
["","","Iekštelpu ierīce-iekštelpu ierīce","Maks.","m","0.5","0.5","0.5","0.5","0.5","0.5","0.5","0.5"]
["Standard Accessories","Installation manual","","","","1","1","1","1","1","1","1","1"]
["","Refrigerant label for F-gas regulation","","","","1","1","1","1","1","1","1","1"]
["","General safety precautions","","","","1","1","1","1","1","1","1","1"]
["","Peel off F-gas label","","","","1","1","1","1","1","1","1","1"]
["","Tie-wraps","","","","2","2","2","2","2","2","2","2"]
["Barošanas avots","Fāze","","","","1~","1~","1~","1~","1~","1~","1~","1~"]
["Strāvas padeve","Frekvence","","","Hz","50","50","50","50","50","50","50","50"]
["","Spriegums","","","V","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240"]
["Strāva — 50Hz","Maks. drošinātāja ampēri (MFA)","","","A","20","20","32","32","32","32","32","32"]
["Kompresors","Veids","","","","Hermētiski noblīvēts šūpojošais kompresors","Hermētiski noblīvēts šūpojošais kompresors"]
["Notes","","","","","","","","","(1) - Saskaņā ar ENER Lot 21","(1) - Saskaņā ar ENER Lot 21","(1) - Saskaņā ar ENER Lot 21","(1) - Saskaņā ar ENER Lot 21"]