{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":18,"n_cols":3,"rows_kept":18,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RRDQ-V1"]
[]
[]
[]
[]
["","","RRDQ220V1"]
["Standard Accessories","1/4” uzpildes šļūtene ar lodvārstu (sarkans) 152 cm (AR344)","1/4” uzpildes šļūtene ar lodvārstu (sarkans) 152 cm (AR344)"]
["","1/4” uzpildes šļūtene ar lodvārstu (zils) 152 cm (AR344)","1/4” uzpildes šļūtene ar lodvārstu (zils) 152 cm (AR344)"]
["","Filtrs (TF011)","Filtrs (TF011)"]
["","Sausā filtra kasetne ar molekulāro sietu (AR179E)","Sausā filtra kasetne ar molekulāro sietu (AR179E)"]
["","Skatstikls 1/4\" (ES603)","Skatstikls 1/4\" (ES603)"]
["","Izjaucams savienojums, 1/4” iekšējā vītne x 1/4” iekšējā vītne (BF0020)","Izjaucams savienojums, 1/4” iekšējā vītne x 1/4” iekšējā vītne (BF0020)"]
["","Lietošanas rokasgrāmata RRDQ220V1 (IM0496)","Lietošanas rokasgrāmata RRDQ220V1 (IM0496)"]
["","Šķidruma uzpildes adapteris 1/4” — izmanto R134a recirkulācijai (izvēles aprīkojums)","Šķidruma uzpildes adapteris 1/4” — izmanto R134a recirkulācijai (izvēles aprīkojums)"]
["Notes","","(1) - Specifikācijas var tikt mainītas bez iepriekšēja brīdinājuma"]
["","","(2) - Recirkulācijas pakāpe dažādos apstākļos var atšķirties"]
["","","(3) - R134a recirkulācijai, sekojiet norādījumiem, kas doti lietošanas rokasgrāmatas 11. lappusē"]
["","","(4) - Recirkulācijas rezultāti var atšķirties atkarībā no recirkulētā aukstumaģenta piesārņojuma"]