{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":5,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","WLTRH"]
[]
[]
[]
[]
["","","","","WLTRH."]
["Maksimālais pievienojamo iekštelpu ierīču skaits","","","","0"]
["Maksimālais pievienojamo āra ierīču skaits @","","","","0"]
["Korpuss","Krāsa","","","Balts"]
["","Pogu pārsegs","","","Nē"]
["","Darbības LED","Krāsa","","Zaļš"]
["Izmēri","Ierīce","Augstums","mm","75"]
["","","Platums","mm","60.0"]
["","","Dziļums","mm","25.0"]
["","Ierīce iesaiņojumā","Augstums","mm","380"]
["","","Platums","mm","305"]
["","","Dziļums","mm","195"]
["Svars","Ierīce","","kg","0.036"]
["Iepakojums","Materiāls","","","Pape"]
["","Svars","","kg","0.0084"]
["Vides temperatūra","Darbība","Min.","°C","-10"]
["","","Maks.","°C","50"]
["","Krātuve","Min.","°C","-10"]
["","","Maks.","°C","50"]
["","Vides temperatūra-=-Relatīvais mitrums <-=-%","","%","100"]
["Uzstādīšana","","","","Uzstādīšana iekštelpās"]